{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["2014年移动电源产品风险监测检测结果汇总表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"2014年移动电源产品风险监测检测结果汇总表","index":0,"n_rows":64,"n_cols":16,"rows_kept":64,"merged":[[0,0,0,15]],"flags":["formulas_cached_only"]}
["2014年移动电源产品风险监测检测结果汇总表"]
[]
["序号","规格型号","标称生产企业","外观及尺寸","输出电压和额定输出电流（%）","额定容量(mAh)","静态消耗电流（μA）","转换效率（%）","高温放电(mAh)","低温放电(mAh)","短路保护","放电过流保护","过充电保护","外壳防火等级","振动","外壳温度（℃）"]
[{"$nulls":3},"外观、尺寸、状态指示、标志等符合标准要求","输出电压：95%～105%输出额定电流：≥95%","移动电源放电容量应符合制造商规定（占比）","≤100","≥85%","放电容量值不低于额定容量。（占比）","放电容量值不低于额定容量的60%。（占比）","移动电源应不泄露、不泄气、不破裂、不起火和不爆炸，短路解除后移动电源各项功能正常。","移动电源应不泄露、不泄气、不破裂、不起火和不爆炸。（过流保护值符合制造商规定）","移动电源应不泄露、不泄气、不破裂、不起火和不爆炸，移动电源各项功能正常。","阻燃等级达到V-1的要求。","移动电源应不泄露、不泄气、不破裂、不起火和不爆炸；晃动产品，内部应无声响或明显部件松动，移动电源各项功能正常。","外壳温度应不超过允许的温度上限Tlmt（室温23℃时塑料外壳为73℃；金属壳为53℃）"]
[1,"L10","深圳忆捷创新科技有限公司","不符合标准要求","输出电压：93%～103%\n输出额定电流：100%","6379（61%）",52.1,{"v":0.88,"d":"88%"},"6381（61%）","5677（55%）","符合要求","符合要求(5.5A/5.5A)","符合要求","非阻燃","符合要求",36.6]
[2,"E10A","深圳市欧度利方科技有限公司","不符合标准要求","输出电压：100%～104%\n输出额定电流：100%","6297（63%）",50,{"v":0.78,"d":"78%"},"6294（63%）","5593（56%）","符合要求","符合要求(5.5A/5.5A)","符合要求","金属外壳","符合要求",32.7]
[3,"EB-PG900B","三星电子（越南）有限公司","不符合标准要求","输出电压：97%～101%\n输出额定电流：100%","3918（65%）",224.9,{"v":0.87,"d":"87%"},"3922（65%）","3488（58%）","符合要求","符合要求(3.5A/——)","符合要求","非阻燃","符合要求",40.3]
[4,"移动家源N20","深圳市迪比科电子科技有限公司","不符合标准要求","输出电压：100%～103%\n输出额定电流：100%","12777（64%）",52.5,{"v":0.9,"d":"90%"},"12753（64%）","11341（57%）","符合要求","符合要求(5.5A/5.5A)","符合要求","阻燃","符合要求",33.7]
[5,"NDY-02-AD","江苏紫米电子技术有限公司","不符合标准要求","输出电压：93%～103%\n输出额定电流：100%","6977（67%）",458.2,{"v":0.85,"d":"85%"},"6977（67%）","6191（60%）","符合要求","符合要求(5.0A/——)","符合要求","金属外壳","符合要求",36.7]
[6,"E10","北京小菜网络科技有限公司","不符合标准要求","输出电压：84%～103%\n输出额定电流：100%","3271（33%）",11.5,{"v":0.79,"d":"79%"},"3275（33%）","2924（29%）","符合要求","符合要求(4.0A/——)","符合要求","非阻燃","符合要求",41.7]
[7,"M10400C","深圳市万拓电子技术有限公司","不符合标准要求","输出电压：97%～103%\n输出额定电流：100%","6836（66%）",14.9,{"v":0.82,"d":"82%"},"6821（66%）","6066（58%）","符合要求","符合要求(4.8A/4.8A)","符合要求","阻燃","符合要求",39.3]
[8,"P48","深圳市广源华科技有限公司","不符合标准要求","输出电压：95%～101%\n输出额定电流：100%","12307（62%）",54.6,{"v":0.8,"d":"80%"},"12294（61%）","10917（55%）","符合要求","符合要求(5.5A/5.5A)","符合要求","金属外壳","符合要求",33.8]
[9,"P40","深圳市广源华科技有限公司","不符合标准要求","输出电压：96%～104%\n输出额定电流：100%","7348（61%）",5,{"v":0.78,"d":"78%"},"7341（61%）","6838（57%）","符合要求","符合要求(3.0A/3.0A)","符合要求","金属外壳","符合要求",37.9]
[10,"SPB-M100","飞毛腿电池有限公司","不符合标准要求","输出电压：96%～101%\n输出额定电流：100%","7522（75%）",82.7,{"v":0.92,"d":"92%"},"7526（75%）","6703（67%）","符合要求","符合要求(3.0A/3.0A)","符合要求","金属外壳","符合要求",32.7]
[11,"SPB-M60","飞毛腿电池有限公司","不符合标准要求","输出电压：97%～101%\n输出额定电流：100%","4474（72%）",85.5,{"v":0.93,"d":"93%"},"4481（72%）","3984（64%）","符合要求","符合要求(4.3A/——)","符合要求","非阻燃","符合要求",43.7]
[12,"TS-D132","广东品胜电子股份有限公司","不符合标准要求","输出电压：97%～102%\n输出额定电流：100%","3036（61%）",21.5,{"v":0.79,"d":"79%"},"3044（61%）","2653（53%）","符合要求","符合要求(4.3A/——)","符合要求","非阻燃","符合要求",47.3]
[13,"TS-D182","广东品胜电子股份有限公司","不符合标准要求","输出电压：98%～102%\n输出额定电流：100%","6118（61%）",9.6,{"v":0.77,"d":"77%"},"6120（61%）","5503（55%）","符合要求","符合要求(5.5A/5.5A)","符合要求","阻燃","符合要求",31.7]
[14,"PH80","深圳市力可普尔电子有限公司","不符合标准要求","输出电压：94%～100%\n输出额定电流：100%","10918（55%）","2.58mA",{"v":0.82,"d":"82%"},"10913（55%）","9684（48%）","符合要求","符合要求(5.5A/5.5A)","符合要求","非阻燃","符合要求",35.4]
[15,"PH50","深圳市力可普尔电子有限公司","不符合标准要求","输出电压：96%～100%\n输出额定电流：100%","6657（64%）",37.4,{"v":0.82,"d":"82%"},"6364（61%）","6119（59%）","符合要求","符合要求(5.5A/5.5A)","符合要求","非阻燃","符合要求",38.6]
[16,"V86","上海熊剑信息科技有限公司","不符合标准要求","输出电压：98%～104%\n输出额定电流：100%","4304（41%）",23.2,{"v":0.78,"d":"78%"},"4315（41%）","3807（37%）","符合要求","符合要求(2.6A/2.6A)","符合要求","非阻燃","符合要求",32.7]
[17,"U14000","南京华旗资讯科技有限公司","不符合标准要求","输出电压：95%～103%\n输出额定电流：100%","8325（59%）",97,{"v":0.76,"d":"76%"},"8317（59%）","7369（53%）","符合要求","符合要求(2.5A/——)","符合要求","非阻燃","符合要求",33.5]
[18,"P3","深圳市华美兴泰科技有限公司","不符合标准要求","输出电压：98%～103%\n输出额定电流：100%","2752（55%）",64.5,{"v":0.76,"d":"76%"},"2742（55%）","2219（44%）","符合要求","符合要求(19A/19A)","符合要求","金属外壳","符合要求",39.4]
[19,"P6","深圳市华美兴泰科技有限公司","不符合标准要求","输出电压：100%～104%\n输出额定电流：100%","6140（59%）",63.6,{"v":0.73,"d":"73%"},"6127（59%）","5419（52%）","符合要求","符合要求(4.3A/4.3A)","符合要求","金属外壳","符合要求",33.5]
[20,"DLP2052","沃科声（上海）商贸有限公司","不符合标准要求","输出电压：98%～103%\n输出额定电流：100%","3214（62%）",18.2,{"v":0.77,"d":"77%"},"3220（62%）","2853（55%）","符合要求","符合要求(19A/19A)","符合要求","金属外壳","符合要求",36.2]
[21,"HB-T10","深圳市哈里通实业有限公司","不符合标准要求","输出电压：99%～101%\n输出额定电流：100%","5783（58%）","3.28mA",{"v":0.76,"d":"76%"},"5767（58%）","5119（51%）","符合要求","符合要求(5.5A/5.5A)","符合要求","金属外壳","符合要求",38.6]
[22,"格子G10","深圳市迪比科电子科技有限公司","不符合标准要求","输出电压：94%～101%\n输出额定电流：100%","5967（60%）",19.4,{"v":0.79,"d":"79%"},"5961（60%）","5261（53%）","符合要求","符合要求(未测出/未测出)","符合要求","阻燃","符合要求",33]
[23,"KBC-L2BC-S","松下电器（中国）有限公司","不符合标准要求","输出电压：96%～104%\n输出额定电流：100%","2665（53%）",15,{"v":0.72,"d":"72%"},"2671（53%）","2381（48%）","符合要求","符合要求(9.5A/9.5A)","符合要求","阻燃","符合要求",40.4]
[24,"FD-PB15","深圳商斯迈科技有限公司","不符合标准要求","输出电压：98%～103%\n输出额定电流：100%","4951（62%）",202.7,{"v":0.83,"d":"83%"},"4982（62%）","4421（55%）","符合要求","符合要求(2.6A/5.1A)","符合要求","非阻燃","符合要求",42.7]
[25,"WT105","北京纽曼腾飞科技有限公司","不符合标准要求","输出电压：50%～104%\n输出额定电流：100%","6425（64%）",31.1,{"v":0.8,"d":"80%"},"6446（64%）","5716（57%）","符合要求","符合要求(3.5A/3.5A)","符合要求","非阻燃","符合要求",33.7]
[26,"XP-2W","深圳市奥之博科技有限公司","不符合标准要求","输出电压：88%～104%\n输出额定电流：100%","6543（33%）",7.6,{"v":0.75,"d":"75%"},"6547（33%）","5794（29%）","符合要求","符合要求(2.7A/——)","符合要求","非阻燃","符合要求",30.8]
[27,"XP-J12","深圳市奥之博科技有限公司","不符合标准要求","输出电压：98%～103%\n输出额定电流：100%","5408（45%）",28.1,{"v":0.91,"d":"91%"},"5419（45%）","4811（40%）","符合要求","符合要求(6.5A/——)","符合要求","非阻燃","符合要求",41.3]
[28,"LEPOWU-STONE","深圳市乐泡创新科技有限公司","不符合标准要求","输出电压：96%～102%\n输出额定电流：100%","7641（64%）",89.2,{"v":0.81,"d":"81%"},"7633（64%）","6764（56%）","符合要求","符合要求(6.5A/——)","符合要求","非阻燃","符合要求",40.4]
[29,"P15000","太空步（中国）营销总部","不符合标准要求","输出电压：99%～102%\n输出额定电流：100%","6715（45%）",10.4,{"v":0.76,"d":"76%"},"6727（45%）","5961（40%）","符合要求","符合要求(4.8A/3.5A)","符合要求","非阻燃","符合要求",39.8]
[30,"P10","太空步（中国）营销总部","不符合标准要求","输出电压：99%～104%\n输出额定电流：100%","5594（56%）",4.7,{"v":0.77,"d":"77%"},"5544（55%）","4914（49%）","符合要求","符合要求(5.5A/——)","符合要求","金属外壳","符合要求",38.6]
[31,"X-44C","广州市顺风电子科技有限公司","不符合标准要求","输出电压：98%～99%\n输出额定电流：100%","2757（63%）",54.3,{"v":0.87,"d":"87%"},"2644（60%）","1795（41%）","符合要求","符合要求（2.8A/——）","符合要求","非阻燃","符合要求",43.4]
[32,"无","广州市天地星电讯有限公司","不符合标准要求","输出电压:95%~102%\n输出额定电流:100%","1884（65%）",11.2,{"v":0.81,"d":"81%"},"1892（65%）","1312（45%）","符合要求","符合要求（2.7A/——）","符合要求","阻燃","符合要求",36.6]
[33,"F5000","南京华旗资讯科技有限公司","不符合标准要求","输出电压:99%-110%\n输出额定电流:100%","2614（52%）",98.8,{"v":0.848,"d":"84.80%"},"2886（58%）","2348（47%）","符合要求","符合要求（1.9A/——）","符合要求","阻燃","符合要求",41.1]
[34,"Z10000","南京华旗资讯科技有限公司","不符合标准要求","输出电压:90%-92%\n输出额定电流：100%","6060（61%）",83.3,{"v":0.76,"d":"76%"},"5826（58%）","3955（40%）","符合要求","符合要求（3.5A/3.5A）","符合要求","金属外壳","符合要求",41.2]
[35,"T100I-W","广州商科信息技术有限公司","不符合标准要求","输出电压:97%-98%\n输出额定电流:100%","6358（64%）",78.2,{"v":0.89,"d":"89%"},"6544（65%）","4598（46%）","符合要求","符合要求(1.4A/——)","符合要求","阻燃","符合要求",32.9]
[36,"D5200","爱国者电子科技有限公司","不符合标准要求","输出电压65%-102%\n输出额定电流:100%","3685（71%）",27.7,{"v":0.84,"d":"84%"},"3586（69%）","2378（46%）","符合要求","符合要求(2.5A/——)","符合要求","阻燃","符合要求",42]
[37,"D12","爱国者电子科技有限公司","不符合标准要求","输出电压:99%-100%\n输出额定电流:100%","6410（64%）",16.2,{"v":0.91,"d":"91%"},"6586（66%）","4340（43%）","符合要求","符合要求(2.6A/——)","符合要求","非阻燃","符合要求",39.3]
[38,"T&F-72","深圳市同方多媒体科技有限公司","不符合标准要求","输出电压:95%-98%\n输出额定电流:100%","3904（39%）",13.5,{"v":0.81,"d":"81%"},"4225（42%）","3059（31%）","符合要求","符合要求(2.5A/2.7A)","符合要求","非阻燃","符合要求",50.8]
[39,"PD502","奥海集团（香港）有限公司","不符合标准要求","输出电压:97%-100%\n输出额定电流:100%","3086（59%）",60.3,{"v":0.88,"d":"88%"},"3227（62%）","2354（45%）","符合要求","符合要求(1.2A/——)","符合要求","阻燃","符合要求",37.9]
[40,"QG650","乾冠（香港）科技有限公司","不符合标准要求","输出电压:95%-96%\n输出额定电流:100%","5455（55%）",98,{"v":0.82,"d":"82%"},"5250（53%）","3500（35%）","符合要求","符合要求(1.7A/2.3A)","符合要求","金属外壳","符合要求",32.7]
[41,"JW-A6X","深圳市途歌电子有限公司","不符合标准要求","输出电压:97%-98%\n输出额定电流:100%","3083（51%）",71.8,{"v":0.86,"d":"86%"},"2765（46%）","2380（40%）","符合要求","符合要求(2.4A/——)","符合要求","非阻燃","符合要求",58.7]
[42,"未标出","睿丰实业（亚洲）有限公司","不符合标准要求","输出电压:99%-100%\n输出额定电流:100%","3703（74%）",6.9,{"v":0.88,"d":"88%"},"3675（75%）","2428（49%）","符合要求","符合要求(2.2A/——)","符合要求","金属外壳","符合要求",31.2]
[43,"未标出","睿丰实业（亚洲）有限公司","不符合标准要求","输出电压:99%-100%\n输出额定电流:100%","6816（68%）",2.52,{"v":0.77,"d":"77%"},"6486（65%）","4347（43%）","符合要求","符合要求(2.4A/2.5A)","符合要求","金属外壳","符合要求",31.7]
[44,"S3","深圳市锐讯天成科技有限公司\n羽博国际集团（香港）有限公司 出品","不符合标准要求","输出电压:99%-100%\n输出额定电流:100%","3831（64%）",53.6,{"v":0.86,"d":"86%"},"3900（65%）","2700（45%）","符合要求","符合要求(2.3A/——)","符合要求","金属外壳","符合要求",33.6]
[45,"PD504","奥海集团（香港）有限公司","不符合标准要求","输出电压:97%-99%\n输出额定电流:100%","6639（64%）",55.3,{"v":0.87,"d":"87%"},"6765（65%）","5050（49%）","符合要求","符合要求(2.8A/——)","符合要求","阻燃","符合要求",38.6]
[46,"YB-655","深圳市锐讯天成科技有限公司\n羽博国际集团（香港）有限公司 出品","不符合标准要求","输出电压：96%-97%\n输出额定电流:100%","7064（64%）",42.4,{"v":0.85,"d":"85%"},"7198（65%）","5443（49%）","符合要求","符合要求(2.2A/——)","符合要求","阻燃","符合要求",32.7]
[47,"YB-665","深圳市锐讯天成科技有限公司\n羽博国际集团（香港）有限公司 出品","不符合标准要求","输出电压:92%-94%\n输出额定电流:100%","10086（65%）",1030,{"v":0.83,"d":"83%"},"9872（63%）","7617（49%)","符合要求","符合要求(2.3A/3.4A)","符合要求","阻燃","符合要求",43.2]
[48,"EMIE-ES100-C","深圳市亿觅科技有限公司","不符合标准要求","输出电压:97%-98%\n输出额定电流:100%","4717（59%）",2770,{"v":0.81,"d":"81%"},"4869（61%）","2955（37%）","符合要求","符合要求(2.8A/——)","符合要求","非阻燃","符合要求",67.1]
[49,"BST-0137","深圳市倍斯特电源有限公司","不符合标准要求","输出电压:98%-100%\n输出额定电流:100%","7905（66%）",422.6,{"v":0.87,"d":"87%"},"7822（65%）","5608（47%）","符合要求","符合要求(4.5A/——)","符合要求","非阻燃","符合要求",33.5]
[50,"GPB-B0060R","睿米国际（香港）有限公司","不符合标准要求","输出电压:96%-97%\n输出额定电流:100%","3878（65%）",53.4,{"v":0.86,"d":"86%"},"3675（61%）","2572（43%）","符合要求","符合要求(2.4A/——)","符合要求","金属外壳","符合要求",31.2]
[51,"K16","深圳市嘉松伟业科技有限公司","不符合标准要求","输出电压:97%-104%\n输出额定电流:100%","9348（58%）",181.2,{"v":0.8,"d":"80%"},"6654（42%）","5366（34%）","符合要求","符合要求(2.5A/2.6A)","符合要求","非阻燃","符合要求",58.6]
[52,"SRBC535","深圳市大乘科技有限公司","不符合标准要求","输出电压:96%-100%\n输出额定电流:100%","4242（64%）",93,{"v":0.88,"d":"88%"},"4326（66%）","3393（51%）","符合要求","符合要求(1.6A/——)","符合要求","非阻燃","符合要求",33]
[53,"SRBC536","深圳市大乘科技有限公司","不符合标准要求","输出电压:97%-99%\n输出额定电流:100%","7559（69%）",97.9,{"v":0.84,"d":"84%"},"6970（63%）","5420（49%）","符合要求","符合要求(2.4A/2.5A)","符合要求","非阻燃","符合要求",49.4]
[54,"PA10400","联想（北京）有限公司","不符合标准要求","输出电压:96%-97%\n输出额定电流:100%","6348（61%）",9.4,{"v":0.85,"d":"85%"},"6818（66%）","5140（49%）","符合要求","符合要求(2.2A/2.2A)","符合要求","非阻燃","符合要求",42.7]
[55,"PA7800","联想（北京）有限公司","不符合标准要求","输出电压:95%-97%\n输出额定电流:100%","4737（61%）",9.9,{"v":0.85,"d":"85%"},"5145（66%）","3884（50%）","符合要求","符合要求(2.3A/——)","符合要求","非阻燃","符合要求",53.1]
[56,"CP-F5","索尼（中国）有限公司","不符合标准要求","输出电压:98%-99%\n输出额定电流:100%","3106（104%）",28.5,{"v":0.85,"d":"85%"},"3075（102%）","2040（68%）","符合要求","符合要求(2.0A/——)","符合要求","金属外壳","符合要求",30.8]
[57,"A10000","深圳市图美电子技术有限公司","不符合标准要求","输出电压:86%-95%\n输出额定电流:100%","6406（64%）",59.4,{"v":0.81,"d":"81%"},"5960（60%）","5318（53%）","符合要求","符合要求(2.7A/——)","符合要求","非阻燃","符合要求",54.3]
[58,"CS5200","深圳市七彩虹科技发展有限公司","不符合标准要求","输出电压:99%-101%\n输出额定电流:100%","3121（60%）",4.8,{"v":0.87,"d":"87%"},"3333（64%）","2686（52%）","符合要求","符合要求(2.0A/——)","符合要求","阻燃","符合要求",40.4]
[59,"PN-918","中山市品能电池有限公司 品能国际（香港）有限公司出品","不符合标准要求","输出电压:95%-99%\n输出额定电流:100%","5376（54%）",184.4,{"v":0.82,"d":"82%"},"6100（102%）","4742（79%）","符合要求","符合要求(1.3A/——)","符合要求","阻燃","符合要求",39.8]
[60,"TP-U101","深圳市创世达实业有限公司","不符合标准要求","输出电压:97%-98%\n输出额定电流:100%","6567（63%）",12.9,{"v":0.79,"d":"79%"},"6336（61%）","5344（51%）","符合要求","符合要求(2.4A/2.4A)","符合要求","阻燃","符合要求",50.6]